For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear wheel bearing/hub assembly. Refer to Rear Wheel Bearing and Hub Replacement .

1 | Wheel Stud (Qty: 6)

#### Procedure

1. Use either an old lug nut or a nut that will fit the wheel stud.
2. Tighten the lug nut/nut until the wheel stud is seated against the wheel hub.

Tip
Ensure that the washers being used, the center hole is larger than the wheel stud.

#### Special Tools

J 43631 Ball Joint Remover