For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement.

1 | Front Seat Cushion Frame Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
2 | Front Seat Cushion Frame

#### Procedure

Disengage the springs from the seat cushion frame.