For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove rear seat. Refer to Rear Seat Replacement.
2. Remove seat back pad and cover. Refer to Rear Seat Cushion Cover and Pad Replacement.

1 | Rear Seat Center Belt Retractor Assembly Tip Tilt 40 percent split forward for access.
2 | Rear Seat Center Belt Retractor Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 52 N·m (38 lb ft)
3 | Rear Seat Center Belt Assembly