For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the front floor console. Refer to Front Floor Console Replacement.
3. Remove HVAC floor duct.
4. Position carpet in order to access sensor.
5. Disconnect the electrical connector.

1 | Inflatable Restraint Sensor and Diagnostic Module Nut (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (88 lb ft)
2 | Inflatable Restraint Sensor and Diagnostic Module Assembly

#### Procedure

1. When installing, ensure the arrow on the module is pointed towards the front of the vehicle.
2. If installing a replacement module, program the module. Refer to Control Module References.