For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the EVAP canister. Refer to Evaporative Emission Canister Replacement .
2. Remove the foam pad insulators.

1 | Fuel Tank
2 | Evaporative Emission Canister Vent Rear Pipe

#### Procedure

1. Disconnect the quick connect fitting from the fuel tank module. Refer to Plastic Collar Quick Connect Fitting Service .
2. Disconnect the quick connect fittings from the rollover valves. Refer to Plastic Collar Quick Connect Fitting Service .
3. Disengage from the tank retaining features.