For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Disconnect the body wire harness (2) from the trailer wire harness connector (1).
3. If replacing the trailer hitch, remove the trailer wire harness connector (1) from the trailer hitch (2).
4. Remove the trailer hitch bolts (2-4).
5. Remove the trailer hitch (1).

### Installation Procedure

1. Install the trailer hitch (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the trailer hitch bolts (2-4).

Tighten
Tighten the bolts to 100 N·m (74 lb ft).

3. If previously removed, install the trailer wire harness connector (1) to the trailer hitch (2).
4. Connect the body wire harness (2) to the trailer wire harness connector (1).
5. lower the vehicle.