For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Unzip the side zipper of the rear seat number 2 back cover.
2. Remove the rear seat No. 2 cushion cover and pad. Refer to Rear Seat Number 2 Cushion Cover and Pad Replacement.
3. Remove the recliner inner finish covers. Refer to Rear Seat Number 2 Recliner Inner Finish Cover Replacement.
4. Remove the rear seat number 2 belt buckle. Refer to Rear Seat Number 2 Belt Buckle Replacement.

1 | Rear Seat No. 2 Back Cushion Frame Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Rear Seat No. 2 Riser Bolt (Qty: 3) Tighten 55 N·m (41 lb ft)
3 | Rear Seat No. 2 Back Cushion Hinge Assembly (Qty: 2)