For 1990-2009 cars

## 2-Way Remote Start and Door Lock Transmitter Package Installation BTV (Traverse Only)

### Accessories Part Number

19156554 or 19171129

### Kit Usage

This kit is designed to add 2-way remote start with extended range and enhanced functionality. It is for vehicles equipped with remote vehicle start from the factory (vehicles with option code BTV). If the vehicle is not equipped with remote vehicle start, it does not have the hood switch and wiring required.

#### Kit Contents

Qty | Description
--- | ---
1 | Remote Control Door Lock, 2-Way Remote Start and Information Display Receiver (2-Way RCDLR)
1 | 2-Way Remote Start and Door Lock Transmitter (With Information Display)
1 | 2-Way Remote Start, Door Lock and Information Display Antenna
1 | 2-Way Advanced Remote Start Owner Manual

### Special Tools

• | Scan Tool with capability of communicating on GMLAN

• | Service Programming System (SPS - TIS2WEB or equivalent)

• | J-46079 Tire Pressure Monitor Diagnostic Tool

• | Surface Cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent)

• | Adhesion Promoter GM P/N 12378462 (Canadian P/N 10953554)

### Procedure

Note: Please review this entire procedure before trying to perform it.

1. Using the scan tool, perform the copy and paste TPM information procedure. This will extract the TPM tire type information as well as the sensor data from the existing RCDLR prior to its replacement and store this information in the scan tool. After RCDLR replacement, the tire type and sensor data stored in the scan tool is written to the new RCDLR, negating the need to perform the tire type setup and sensor learn procedure. This must be performed BEFORE removing the old RCDLR. Refer to Remote Control Door Lock Receiver Programming and Setup.
2. Physically replace the factory Remote Control Door Lock Receiver (RCDLR) with the 2-way RCDLR included in the kit. Refer to Remote Control Door Lock Receiver Replacement. Do not program or reassemble yet.

Note: The cargo screen retainer will need to be turned and twisted prior to pulling outward to release. There are two hidden bolts, one under the armrest and one behind the cargo screen retainer.

3. Remove the right rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
4. Measure a=85 mm (3 3/8 in) length of antenna cable from the antenna and secure the antenna cable to the right side quarter inner body structure under the window opening with three adhesive wire-wraps (2). Align the first wire-wrap using b=420 mm (16 1/2 in) from the window locator pin (1).
5. Clean the top surface of the upper auxiliary air distributor duct (4) where the antenna cable will be secured with a surface cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent).
6. Apply adhesion promoter GM P/N 12378462 (Canadian P/N 10953554) to the surface of the duct (4). Follow the adhesion promoter instructions on the product label.
7. Secure the antenna cable to the top of the upper auxiliary air distributor duct (4) with one adhesive wire wrap (2).
8. Secure the antenna cable to the main body harness and headliner harness with four tie wraps (1).
9. Connect the antenna cable to the 2-way RCDLR.
10. Secure the factory antenna connector (2) to the vehicle body structure with one adhesive wire wrap.

Note: Excess antenna cable length must be looped in a "figure 8" no less than 100 mm (4 in) in length for the best performance of the system.

11. Loop any excess antenna cable length into a "figure 8" at least 100 mm (4 in) long and secure to the headliner wiring harness (1) (glued to the headliner (4)) with two tie wraps (2).
12. Clean the surface of the right rear quarter lower trim panel (2) where the antenna (1) will be installed with a surface cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent).
13. Dry the trim panel thoroughly using a lint-free cloth.

Note:

• | The adhesion promoter must be used to assure adequate bonding of the antenna.

• | Mask off or protect areas before applying the adhesion promoter.

14. Apply adhesion promoter GM P/N 12378462 (Canadian P/N 10953554) to the right rear quarter lower trim panel (2) in the area where you will install the antenna (1). Follow the adhesion promoter instructions on the product label, use a=33 mm (1 5/16 mm) and b=184 mm (7 1/4 in) for the dimensions on the figure.

Note:

• | Position the antenna according to the figure provided.

• | Do not touch the adhesive pad on the antenna.

15. Remove the protective film from the adhesive pad on the antenna.
16. Align the antenna according to the figure, using a=33 mm (1 5/16 mm) and b=184 mm (7 1/4 in).
17. Press firmly all along the antenna, including all four corners of the adhesive pad, in order to ensure proper adhesion to the trim panel.
18. Hold pressure on the antenna for 10-30 seconds.
19. Program the new RCDLR. Refer to Remote Control Door Lock Receiver Programming and Setup. Program the 2-way transmitter and the vehicle factory transmitters to the new RCDLR.
20. Turn the ignition off for 1 minute.
21. Turn the ignition on.
22. Using the scan tool, retrieve any diagnostic trouble codes (DTCs) from all of the modules.
23. Clear all DTCs.
24. Remove the scan tool.
25. Operate the 2-way and factory transmitters in order to verify correct system operation. Refer to Keyless Entry System Description and Operation. Press a command button with the vehicle ignition ON in order to synchronize the 2-way transmitter clock to the vehicle clock.
26. Reassemble. Refer to Quarter Lower Rear Trim Panel Replacement.
27. Drive the vehicle at least 1 mile above 25 mph. This is to synchronize the 2-way transmitter odometer display to the vehicle odometer and update the tire pressure displays.
28. Add the transmitters to the customer key rings.
29. Place the 2-Way Advanced Remote Start owner manual in instrument panel compartment.
30. Keep the vehicle dry. Allow 6-8 hours, at 15°C (60°F), for the antenna adhesive to cure after installation.

## 2-Way Remote Start and Door Lock Transmitter Package Installation BTV (Acadia and OUTLOOK Only)

### Accessories Part Number

19156554 or 19171129

### Kit Usage

This kit is designed to add 2-way remote start with extended range and enhanced functionality. It is for vehicles equipped with remote vehicle start from the factory (vehicles with option code BTV). If the vehicle is not equipped with remote vehicle start, it does not have the hood switch and wiring required.

#### Kit Contents

Qty | Description
--- | ---
1 | Remote Control Door Lock, 2-Way Remote Start and Information Display Receiver (2-Way RCDLR)
1 | 2-Way Remote Start and Door Lock Transmitter (With Information Display)
1 | 2-Way Remote Start, Door Lock and Information Display Antenna
1 | 2-Way Advanced Remote Start Owner Manual

### Special Tools

• | Scan Tool with capability of communicating on GMLAN

• | Service Programming System (SPS - TIS2WEB or equivalent)

• | J-46079 Tire Pressure Monitor Diagnostic Tool

• | Surface Cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent)

• | Adhesion Promoter GM P/N 12378462 (Canadian P/N 10953554)

### Procedure

Note: Please review this entire procedure before trying to perform it.

1. Using the scan tool, perform the copy and paste TPM information procedure. This will extract the TPM tire type information as well as the sensor data from the existing RCDLR prior to its replacement and store this information in the scan tool. After RCDLR replacement, the tire type and sensor data stored in the scan tool is written to the new RCDLR, negating the need to perform the tire type setup and sensor learn procedure. This must be performed BEFORE removing the old RCDLR. Refer to Remote Control Door Lock Receiver Programming and Setup.
2. Physically replace the factory remote control door lock receiver (RCDLR) with the 2-way RCDLR included in the kit. Refer to Remote Control Door Lock Receiver Replacement. Do not program or reassemble yet.

Note: To remove the right rear quarter lower trim panel, the cargo screen retainer will need to be turned and twisted prior to pulling outward to release. There are two hidden bolts, one under the armrest and one behind the cargo screen retainer.

3. Remove the right body lock pillar upper trim panel. Refer to Body Lock Pillar Upper Trim Panel Replacement.
4. Measure 85 mm (3 3/8 in) (a) length of antenna cable from the antenna and secure the cable to the right side quarter inner upper body structure at the window opening with one adhesive wire wrap (1). Align the adhesive wire-wrap with the existing hole in the quarter inner upper body structure (2).
5. Secure the antenna cable to the right side quarter inner lower body structure under the window opening with four adhesive wire-wraps (1).
6. Clean the top surface of the upper auxiliary air distributor duct (4) where the antenna cable will be secured with a surface cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent).
7. Apply Adhesion Promoter GM P/N 12378462 (Canadian P/N 10953554) to the surface of duct. Follow the instructions on the product label.
8. Secure the antenna cable to the top of the upper auxiliary air distributor duct (4) with one adhesive wire-wrap (2).
9. Secure the antenna cable to the main body harness and headliner harness with four tie wraps (1).
10. Connect the antenna cable to the 2-Way RCDLR (1).
11. Secure the factory antenna connector (2) to the vehicle body structure with duct tape.

Note: Excess antenna cable length must be looped in a "Figure 8" no less than 100 mm (4 in) length for the best performance of the system.

12. Loop any excess antenna cable length into a "figure 8" at least 100 mm (4 in) long and secure to the headliner wiring harness (1) (glued to the headliner (4)) with two tie wraps (2).
13. Clean the surface of the right body lock pillar upper trim panel (1) where the antenna (2) will be installed with a surface cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent).
14. Dry the trim panel thoroughly using a lint free cloth.

Note:

• | The adhesion promoter must be used to assure adequate bonding of the antenna.

• | Mask off or protect areas before applying the adhesion promoter.

15. Apply Adhesion Promoter GM P/N 12378462 (Canadian P/N 10953554) to the right body lock pillar upper trim panel (1) in the area where you will install the antenna (2). Follow the adhesion promoter instructions on the product label. Use a=28 mm (1 1/8 in) and b=180 mm (7 1/16 in) for the dimensions on the figure.

Note:

• | Position the antenna according to the figure provided.

• | Do not touch the adhesive pad on the antenna.

16. Remove the protective film from the adhesive pad on the antenna.
17. Align the antenna according to the figure, using a=28 mm (1 1/8 in) and b=180 mm (7 1/16 in).
18. Press firmly all along the antenna, including all four corners of the adhesive pad, in order to ensure proper adhesion to the trim panel.
19. Hold pressure on the antenna for 10-30 seconds.
20. Reassemble. Refer to Body Lock Pillar Upper Trim Panel Replacement and Remote Control Door Lock Receiver Replacement.
21. Program the 2-way RCDLR. Refer to Remote Control Door Lock Receiver Programming and Setup. Program the 2-way transmitter and the vehicle factory transmitters to the 2-way RCDLR.
22. Turn the ignition off for 1 minute.
23. Turn the ignition on.
24. Using the scan tool, retrieve any diagnostic trouble codes (DTCs) from all of the modules.
25. Clear all DTCs.
26. Remove the scan tool.
27. Operate the 2-way and factory transmitters in order to verify correct system operation. Refer to Keyless Entry System Description and Operation. Press a command button with the vehicle ignition ON in order to synchronize the 2-Way transmitter clock to the vehicle clock.
28. Drive the vehicle at least 1 mile above 25 mph. This is to synchronize the 2-Way transmitter odometer display to the vehicle odometer and update the tire pressure displays.
29. Add the transmitters to the customer key rings.
30. Place the 2-Way Advanced Remote Start owner manual in instrument panel compartment.
31. Keep the vehicle dry. Allow 6-8 hours, at 15°C (60°F), for the antenna adhesive to cure after installation.

## 2-Way Remote Start and Door Lock Transmitter Package Installation BTV (Enclave Only)

### Accessories Part Number

19156554

### Kit Usage

This kit is designed to add 2-way remote start with extended range and enhanced functionality. It is for vehicles equipped with remote vehicle start from the factory (vehicles with option code BTV). If the vehicle is not equipped with remote vehicle start, it does not have the hood switch and wiring required.

#### Kit Contents

Qty | Description
--- | ---
1 | Remote Control Door Lock, 2-Way Remote Start and Information Display Receiver (2-Way RCDLR)
1 | 2-Way Remote Start and Door Lock Transmitter (With Information Display)
1 | 2-Way Remote Start, Door Lock and Information Display Antenna
1 | 2-Way Advanced Remote Start Owner Manual

### Special Tools

• | Scan Tool with capability of communicating on GMLAN

• | Service Programming System (SPS - TIS2WEB or equivalent)

• | J-46079 Tire Pressure Monitor Diagnostic Tool

• | Surface Cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent)

• | Adhesion Promoter GM P/N 12378462 (Canadian P/N 10953554)

### Procedure

Note: Please review this entire procedure before trying to perform it.

1. Using the scan tool, perform the copy and paste TPM information procedure. This will extract the TPM tire type information as well as the sensor data from the existing RCDLR prior to its replacement and store this information in the scan tool. After RCDLR replacement, the tire type and sensor data stored in the scan tool is written to the new RCDLR, negating the need to perform the tire type setup and sensor learn procedure. This must be performed BEFORE removing the old RCDLR. Refer to Remote Control Door Lock Receiver Programming and Setup.
2. Physically replace the factory remote control door lock receiver (RCDLR) with the 2-way RCDLR included in the kit. Refer to Remote Control Door Lock Receiver Replacement. Do not program or reassemble yet.

Note: The cargo screen retainer will need to be turned and twisted prior to pulling outward to release. There are two hidden bolts, one under the armrest and one behind the cargo screen retainer.

3. Remove the right rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement.
4. Measure 85 mm (3 3/8 in) (a) length of antenna cable from the antenna and secure the cable (3) to the right side quarter inner body structure under the window opening with three adhesive wire-wraps (2). Align the first wire-wrap with the existing hole and boss on the quarter inner body structure (1).
5. Clean the top surface of the upper auxiliary air distributor duct (4) where the antenna cable will be secured with a surface cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent).
6. Apply adhesion promoter GM P/N 12378462 (Canadian P/N 10953554) to the surface of the duct (4). Follow the adhesion promoter instructions on the product label.
7. Secure the antenna cable to the top of the upper auxiliary air distributor duct (4) with one adhesive wire wrap (2).
8. Secure the antenna cable to the main body harness and headliner harness with four tie wraps (1).
9. Connect the antenna cable to the 2-way RCDLR.
10. Secure the factory antenna connector (2) to the vehicle body structure with one adhesive wire wrap.

Note: Excess antenna cable length must be looped in a "figure 8" no less than 100 mm (4 in) in length for the best performance of the system.

11. Loop any excess antenna cable length into a "figure 8" at least 100 mm (4 in) long and secure to the headliner wiring harness (1) (glued to the headliner (4)) with two tie wraps (2).
12. Clean the surface of the right rear quarter lower trim panel (2) where the antenna (1) will be installed with a surface cleaner (50 percent isopropyl alcohol, FS-1082 hi-flash naphtha or equivalent).
13. Dry the trim panel thoroughly using a lint-free cloth.

Note:

• | The adhesion promoter must be used to assure adequate bonding of the antenna.

• | Mask off or protect areas before applying the adhesion promoter.

14. Apply adhesion promoter GM P/N 12378462 (Canadian P/N 10953554) to the right rear quarter lower trim panel (2) in the area where you will install the antenna (1). Follow the adhesion promoter instructions on the product label, use a=27 mm (1 1/16 in) and b=385 mm (15 3/16 in).

Note:

• | Position the antenna according to the figure provided.

• | Do not touch the adhesive pad on the antenna.

15. Remove the protective film from the adhesive pad on the antenna.
16. Align the antenna according to the figure, using a=27 mm (1 1/16 in) and b=385 mm (15 3/16 in).
17. Press firmly all along the antenna, including all four corners of the adhesive pad, in order to ensure proper adhesion to the trim panel.
18. Hold pressure on the antenna for 10-30 seconds.
19. Reassemble. Refer to Quarter Lower Rear Trim Panel Replacement and Remote Control Door Lock Receiver Replacement.
20. Program the new RCDLR. Refer to Remote Control Door Lock Receiver Programming and Setup. Program the 2-way transmitter and the vehicle factory transmitters to the new RCDLR.
21. Turn the ignition off for 1 minute.
22. Turn the ignition on.
23. Using the scan tool, retrieve any diagnostic trouble codes (DTCs) from all of the modules.
24. Clear all DTCs.
25. Remove the scan tool.
26. Operate the 2-way and factory transmitters in order to verify correct system operation. Refer to Keyless Entry System Description and Operation. Press a command button with the vehicle ignition ON in order to synchronize the 2-way transmitter clock to the vehicle clock.
27. Drive the vehicle at least 1 mile above 25 mph. This is to synchronize the 2-way transmitter odometer display to the vehicle odometer and update the tire pressure displays.
28. Add the transmitters to the customer key rings.
29. Place the 2-way advanced remote start owner manual in the instrument panel compartment.
30. Keep the vehicle dry. Allow 6-8 hours, at 15°C (60°F), for the antenna adhesive to cure after installation.