For 1990-2009 cars

## Rear Seat Back Cushion Frame Replacement With 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.
3. Remove the rear seat latch release handle assembly. Refer to Rear Seat Back Cushion Latch Release Handle Replacement.
4. Remove the rear seat back cushion stowage latch actuator. Refer to Rear Seat Back Cushion Stowage Latch Actuator Replacement.

1 | Rear Seat Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tip Use a grease pencil or marker to mark the location of the bolts for installation to ensure correct alignment of the seat back. Tighten
45 N·m (33 lb ft)

2 | Rear Seat Bolt Tip Use a grease pencil or marker to mark the location of the bolts for installation to ensure correct alignment of the seat back. Tighten 28 N·m (21 lb ft)
3 | Rear Seat Recliner Bolt Tip Use a grease pencil or marker to mark the location of the bolts for installation to ensure correct alignment of the seat back. Tighten 28 N·m (21 lb ft)
4 | Rear Seat Back Frame

## Rear Seat Back Cushion Frame Replacement With 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.
3. Remove the rear seat latch release handle assembly. Refer to Rear Seat Back Cushion Latch Release Handle Replacement.
4. Remove the rear seat back cushion stowage latch actuator. Refer to Rear Seat Back Cushion Stowage Latch Actuator Replacement.

1 | Rear Seat Bolt Caution: Refer to Fastener Caution in the Preface section. Tip Use a grease pencil or marker to mark the location of the bolts for installation to ensure correct alignment of the seat back. Tighten
21 N·m (15 lb ft)

2 | Rear Seat Pivot Bolt Tip Use a grease pencil or marker to mark the location of the bolts for installation to ensure correct alignment of the seat back. Tighten 28 N·m (21 lb ft)
3 | Rear Seat Pivot Bolt Grommet Tip Replace the grommet with a new one whenever the bolt is removed.
4 | Rear Seat Recliner Bolt (Qty: 2) Tip Use a grease pencil or marker to mark the location of the bolts for installation to ensure correct alignment of the seat back. Tighten 45 N·m (33 lb ft)
5 | Rear Seat Back Frame