For 1990-2009 cars

## Hazard Warning Switch Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.

1 | Hazard Warning Switch Assembly

#### Procedure

Disconnect the electrical connector.

## Hazard Warning Switch Replacement Enclave/Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.

1 | Hazard Warning Switch Assembly

#### Procedure

1. Release tab on top and bottom of switch to remove.
2. Disconnect Electrical Connector.

## Hazard Warning Switch Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.

1 | Hazard Warning Switch Assembly

#### Procedure

Disconnect the electrical connector.