For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the inflatable restraint steering wheel module coil. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement.

1 | Turn Signal Switch Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Turn Signal Switch Bracket

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Release the plastic retaining tabs to release the turn signal switch bracket from the steering column.