For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Disable the SIR system. Refer to SIR Disabling and Enabling.

1 | Windshield Side Garnish Molding Screw Caution: Refer to Fastener Caution in the Preface section. Tip Open the access door to remove the screw. Tighten
2 N·m (18 lb in)

2 | Windshield Side Garnish Molding Assembly

#### Procedure

Disconnect the electrical connector.