For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Rear Wheelhouse Liner Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Wheelhouse Liner Plastic Retainer (Qty: 3)
3 | Rear Wheelhouse Liner

#### Procedure

Install using the reverse procedure, with the proper alignment of the rear wheelhouse liner.