For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the frame brace. Refer to Frame Brace Replacement.
3. Remove the heated oxygen sensors. Refer to Heated Oxygen Sensor Replacement - Bank 1 Sensor 2 and Heated Oxygen Sensor Replacement - Bank 2 Sensor 2.

1 | Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 28 N·m (21 lb ft)
2 | Nut (Qty: 2) Tighten 50 N·m (37 lb ft)
3 | Exhaust Flex Pipe Assembly

#### Procedure

Remove and discard the gaskets.