For 1990-2009 cars

## Rear Seat Back Cushion Stowage Latch Actuator Replacement With 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear Seat Back Cushion Stowage Latch Actuator

#### Procedure

• | Disconnect the cable and note the cable routing for installation.

• | The stowage latch actuator housing must be located over the latch release handle cable.

• | The white area of the cable must fit into the seat back frame hooks.

## Rear Seat Back Cushion Stowage Latch Actuator Replacement With 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back cushion cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement.

1 | Rear Seat Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear Seat Back Cushion Stowage Latch Actuator

#### Procedure

• | Disconnect the cable and note the cable routing for installation.

• | The stowage latch actuator housing must be located over the latch release handle cable.

• | The white area of the cable must fit into the seat back frame hooks.