For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat No. 2 back cushion cover and pad. Refer to Rear Seat Number 2 Back Cushion Cover and Pad Replacement.
2. Remove the rear seat No. 2 cushion cover and pad. Refer to Rear Seat Number 2 Cushion Cover and Pad Replacement.

1 | Rear Seat No. 2 Back Cushion Latch Release Handle Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
2 | Rear Seat No. 2 Back Cushion Latch Release Handle

#### Procedure

1. Note the routing of the cables for installation.
2. Disconnect the cables from the head restraint and seat latch.