For 1990-2009 cars

## Radiator Upper Grille Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Upper Radiator Grille Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten Hand tighten the screws.
2 | Upper Radiator Grille Tip Release the retainer tabs securing the upper radiator grille to the front bumper fascia.