For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.

1 | Radio Screw (Qty: 4) Caution: Refer to Component Fastener Tightening Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radio Assembly

#### Procedure

1. Disconnect the electrical connector.
2. Disconnect the antenna cable.
3. Reprogram the radio after replacement. Refer to Control Module References .

Tip
When installing the radio verify that the locator pin on the back of the radio is firmly seated in the I/P structure extension.