For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
2. Remove the manual shaft and position switch assembly. Refer to Manual Shift Detent Lever with Shaft Position Switch Assembly Replacement .

1 | Manual Shift Shaft Seal

#### Procedure

• | For seal removal use J 45201 Cooler Line Seal Remover.

• | For seal installation use J-46626 Seal Installer.

• | Lubricate the manual shaft with ATF to prevent damage to the manual shift shaft seal.

#### Special Tools

• | J 45201 Cooler Line Seal Remover

• | J-46626 Seal Installer