For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat No. 2 back cushion cover and pad. Refer to Rear Seat Number 2 Back Cushion Cover and Pad Replacement.
2. Remove the rear seat No. 2 cushion cover and pad. Refer to Rear Seat Number 2 Cushion Cover and Pad Replacement.

1 | Rear Seat No. 2 Back Cushion Frame Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 55 N·m (41 lb ft)
2 | Rear Seat No. 2 Back Cushion Frame