For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement.

1 | Steering Wheel Spoke Cover (Qty: 2) Tip Use gentle pressure to disengage the steering wheel spoke covers from the steering wheel.
2 | Radio Control Switch Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
3 | Radio Control Switch

#### Procedure

Disconnect any electrical connectors as needed.

4 | Cruise Control Switch Bolt (Qty: 2) Tighten 2.5 N·m (22 lb in)
5 | Cruise Control Switch

#### Procedure

Disconnect any electrical connectors as needed.

6 | Horn Switch

#### Procedure

Disconnect any electrical connectors as needed.

Tip
Use gentle pressure to disengage the horn switch from the steering wheel.