For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the air cleaner element. Refer to Air Cleaner Element Replacement .
2. Remove the windshield washer solvent heater. Refer to Windshield Washer Solvent Heater Replacement .

1 | Master Cylinder Fluid Level Sensor

#### Procedure

1. Disconnect the electrical connector.
2. Compress the locking tabs on the sensor to release the sensor from the brake master cylinder reservoir.