For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Lower the rear of the headliner trim panel. Refer to Headlining Trim Panel Replacement .
2. Disconnect the remote control door lock receiver antenna. Refer to Keyless Entry Antenna Replacement .

1 | Remote Control Door Lock Receiver

#### Procedures

1. Disconnect the electrical connector.
2. The module slides and snaps into the body structure.
3. If a replacement module is installed, program the module. Refer to Control Module References .