For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.

1 | Stabilizer Shaft Link Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Use a wrench to keep the stabilizer shaft link from rotating.
2. Remove the upper stabilizer shaft link retaining nut, washer and bushing.
3. Repeat the previous steps on the lower stabilizer shaft retaining nut, washer and bushing.
4. Remove the stabilizer shaft link from the vehicle. Left side shown, right side similar.

Tip
Apply a small amount of penetrating oil on the treads of the stabilizer shaft link prior to removing the retaining nuts.

Tighten
22 N·m (16 lb ft)