For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seat. Refer to Bucket Seat Replacement.
2. Remove the front seat back recliner outer trim panel. Refer to Front Seat Back Recliner Outer Trim Panel Replacement.
3. Remove the front seat back recliner inner trim panel. Refer to Front Seat Back Recliner Inner Trim Panel Replacement.
4. Remove the front seat back cushion cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.
5. Remove the inflatable restraint side impact module. Refer to Driver or Passenger Seat Side Inflatable Restraint Module Replacement.
6. Remove the lumbar system. Refer to Front Seat Lumbar Support Replacement.

1 | Front Seat Back Cushion Frame Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m (37 lb ft)
2 | Front Seat Back Cushion Frame

#### Procedure

Transfer components as necessary.