For 1990-2009 cars

## Windshield Wiper Arm Replacement Traverse

Callout | Component Name
--- | ---
1 | Windshield Wiper Arm Finish Cap (Qty: 2)
2 | Windshield Wiper Arm Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m(18 lb ft)
3 | Windshield Wiper Arm Assembly

#### Procedure

1. Clean the knurls on the wiper motor pivot shaft after the wiper arm has been removed.
2. Hold and align the tips of the front wiper blades to the paint dots on the windshield while securing the nut.
3. Perform a wet wipe and re-check the alignment, adjust if needed.

## Windshield Wiper Arm Replacement Acadia

Callout | Component Name
--- | ---
1 | Windshield Wiper Arm Finish Cap (Qty: 2)
2 | Windshield Wiper Arm Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m(18 lb ft)
3 | Windshield Wiper Arm Assembly

#### Procedure

1. Clean the knurls on the wiper motor pivot shaft after the wiper arm has been removed.
2. Hold and align the tips of the front wiper blades to the paint dots on the windshield while securing the nut.
3. Perform a wet wipe and re-check the alignment, adjust if needed.

## Windshield Wiper Arm Replacement Enclave

Callout | Component Name
--- | ---
1 | Windshield Wiper Arm Finish Cap (Qty: 2) Tip Use a small flat-bladed tool to release the cap from the arm assembly.
2 | Windshield Wiper Arm Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m(18 lb ft)
3 | Windshield Wiper Arm Assembly

#### Procedure

1. Clean the knurls on the wiper motor pivot shaft after the wiper arm has been removed.
2. Hold and align the tips of the front wiper blades to the paint dots on the windshield while securing the nut.
3. Perform a wet wipe and re-check the alignment, adjust if needed.

## Windshield Wiper Arm Replacement OUTLOOK

Callout | Component Name
--- | ---
1 | Wiper Arm Nut Cap (Qty: 2)
2 | Windshield Wiper Arm Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
3 | Windshield Wiper Arm Assembly

#### Procedure

1. Clean the knurls on the wiper motor pivot shaft after the wiper arm has been removed.
2. Hold and align the front wiper blades to the paint dots on the windshield while securing the nut.
3. Perform a wet wipe and re-check the alignment, adjust if needed.