For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Refrigerant Pressure Sensor. Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

• | Hand start the refrigerant pressure sensor to the compressor hose, taking care not to pinch the O-ring and tighten.

• | Remove electrical connector.

Tighten
4 N·m (35 lb in)

2 | O-ring

#### Procedure

Lubricate the refrigerant pressure sensor O-ring with mineral oil.