For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the LF wheelhouse liner in order to access the washer pumps. Refer to Front Wheelhouse Front Liner Replacement.
2. Drain the washer solvent into a clean suitable container.
3. Disconnect the electrical connector.
4. Disconnect the washer pump hose.

1 | Windshield Washer Pump Assembly

#### Procedure

1. Using two flat-bladed tools, at the pump gasket, pry upwards until the washer pump is dislodged from the washer container.
2. Discard the windshield washer pump grommet.