For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the liftgate. Refer to Liftgate Replacement.
2. Drop the rear of the headliner to access the bolts. Refer to Headliner Replacement Headlining Trim Panel Replacement
3. Use a grease pencil to mark the liftgate hinge position to the body prior to removal.

1 | Liftgate Hinge Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Liftgate Hinge

#### Procedure

• | Adjust the liftgate if needed. Refer to Liftgate Adjustment.

• | Inspect the hinge gasket and replace if damaged or torn.