For 1990-2009 cars

### Removal Procedure

1. Remove the engine front cover. Refer to Engine Front Cover Replacement.
2. Remove the spark plugs in order to ease crankshaft/engine rotation. Refer to Spark Plug Replacement.
3. Remove the right bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Removal - Right Side.

### Installation Procedure

1. Install the right bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Installation - Right Side.
2. Install the spark plugs. Refer to Spark Plug Replacement.
3. Install the engine front cover. Refer to Engine Front Cover Replacement.