For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove front floor console. Refer to Front Floor Console Replacement.

1 | Vehicle Yaw Sensor and Lateral Accelerometer Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb ft)
2 | Vehicle Yaw with Vehicle Lateral Accelerometer Sensor Assembly

#### Procedure

Disconnect the electrical connector.