For 1990-2009 cars

Table 1: | Removal
Table 2: | Installation

### Removal

Callout | Component Name
--- | ---
1 | Front Differential Drive Pinion Gear Bearing Tip

• | When removing the front differential drive pinion gear bearing use J 41816-2 step plate .

• | Use J 8433-1 puller bar or equivalent with bolts 2-3/8 x 3 x 24.

#### Special Tools

• | J 8433-1 Puller Bar or equivalent

• | J 22912-B Split Plate Bearing Remover or equivalent

• | J 41816-2 Step Plate

For equivalent regional tools, refer to Special Tools.

### Installation

Callout | Component Name
--- | ---
1 | Front Differential Drive Pinion Gear Bearing Caution: Pressing against the bearing assembly can damage the bearing and cause premature bearing failure.

#### Special Tools

DT-47928 Bearing Installer

For equivalent regional tools, refer to Special Tools.