For 1990-2009 cars

## Windshield Washer Nozzle Replacement Acadia, Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the hood insulator. Refer to Hood Insulator Replacement.
2. Disconnect the windshield washer hose from the nozzles.

1 | Windshield Washer Nozzle (Qty: 2)

#### Procedure

1. If equipped with heated washer nozzles, disconnect the electrical connectors.
2. Pinch the retainers on the washer nozzles.
3. Push the nozzles outward from the hood in order to remove.

## Windshield Washer Nozzle Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the hood insulator. Refer to Hood Insulator Replacement.
2. Disconnect the windshield washer hose from both washer nozzles.

1 | Windshield Washer Nozzle (Qty: 2)

#### Procedure

1. If equipped with heated washer nozzles, disconnect the electrical connectors.
2. Pinch the retainers on the underside of the washer nozzles.
3. Push the nozzles outward from the hood in order to remove.