For 1990-2009 cars

Checks | Causes
--- | ---
2-6 Clutch Assembly |

• | Inspect for damaged or worn 2-6 Clutch Plates (445-447)

• | Inspect for damaged, worn, broken, improper surface finish or sheared splines on the 2-6 clutch backing plate (448)

• | Inspect for damaged or broken 2-6 clutch piston (405) and piston seals damaged, worn or delaminating

• | Inspect for broken or binding 2-6 clutch piston return spring (406)

• | Inspect for broken or disengaged 2-6 Clutch Piston Return Spring Retainer (407)

Reaction Carrier Assembly (467) |

• | Inspect for stripped or sheared splines on the Input Ring Gear

• | Inspect for disengaged or broken Input Ring Gear Retainer