For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove outside rearview mirror. Refer to Power Mirror Replacement.

1 | Front Side Door Outer Sealing Strip Panel Screw Caution: Refer to Fastener Caution in the Preface section. Tip The screw is located in the lower rear of the door frame. Tighten
1.5 N·m (13 lb in)

2 | Front Side Door Outer Sealing Strip Panel

#### Procedures

1. Remove the outer sealing strip by lifting up on the front of the seal and working rearward.
2. When re-installing the outer sealing strip, align the fastener with the locating hole in the door frame.