For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left rear quarter lower trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Remove the liftgate close actuator bracket (if equipped). Refer to Liftgate Close Actuator Bracket Replacement .

1 | Communication Interface Module Bracket

#### Procedure

Disconnect the electrical connectors.

2 | Digital Radio Receiver

#### Procedure

Refer to Control Module References for programming and set up information.

Tip
Pull tab to release the receiver.