For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front fog lamp bezel. Refer to Front Fog Lamp Bezel Replacement.

1 | Daytime Running Lamp Assembly Screw Caution: Refer to Fastener Caution in the Preface section. Tighten (2.5 N·m (22 lb in)
2 | Daytime Running Lamp Assembly

#### Procedure

Rotate the lamp assembly forward and lift upward in order to disengage the lamp tabs from the parking and front fog lamp bracket assembly.

3 | Parking and Front Fog Lamp Bracket