For 1990-2009 cars

## Radio Speaker Amplifier Replacement With UQG

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left side instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.

1 | Radio Speaker Amplifier Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radio Speaker Amplifier Assembly

#### Procedure

Disconnect the electrical connector.

## Radio Speaker Amplifier Replacement With UQA/UQS

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left side instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.

1 | Radio Speaker Amplifier Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radio Speaker Amplifier Assembly

#### Procedure

Disconnect the electrical connector.