For 1990-2009 cars

### Removal Procedure

1. Remove the engine mount strut and bracket. Refer to Engine Mount Strut Replacement - Right Side and Engine Mount Strut Bracket Replacement - Right Side.
2. Disconnect the engine wiring harness electrical connector (8) from the bank 1 intake CMP actuator solenoid valve.
3. Remove the CMP actuator solenoid valve bolt and valve (2).
4. Inspect the CMP actuator solenoid valve seal and replace as necessary.

### Installation Procedure

1. Inspect the CMP actuator solenoid valve seal for damage. Replace the seal if necessary.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the CMP actuator solenoid valve (2) and bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Connect the engine wiring harness electrical connector (8) to the bank 1 intake CMP actuator solenoid valve.
4. Install the engine mount strut and bracket. Refer to Engine Mount Strut Replacement - Right Side and Engine Mount Strut Bracket Replacement - Right Side.