For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the right or left front floor console extension panel. Refer to Front Floor Console Extension Panel Replacement - Right Side or Front Floor Console Extension Panel Replacement - Left Side.
2. Remove the front floor console rear trim plate. Refer to Front Floor Console Rear Trim Panel Replacement.

1 | Front Floor Console Filler Screw (Qty: 1) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Floor Console Filler Panel
3 | Retainer Clip (Qty: 4)