For 1990-2009 cars

Table 1: | Lower and Upper Body Assemble
Table 2: | Channel Plate and Upper Channel Plate Assemble

### Lower and Upper Body Assemble

Callout | Component Name
--- | ---
1 | Control Valve Lower Body Spacer Plate Assembly Tip Inspect the upper channel plate bolt through holes for damage or burnelling. Any damage around the PCS switch feed holes could cause leakage around the PCS switch seals. Replace as necessary.
2 | Control Valve Upper Body Assembly
3 | Control Valve Body Ball Check Valve (Qty: 9)
4 | Control Valve Channel Plate Assembly
5 | Control Valve Body Bolt 6 x 55 (Qty: 1) Caution: Refer to Fastener Caution in the Preface section. Tighten 12 N·m (9 lb ft)

### Channel Plate and Upper Channel Plate Assemble

Callout | Component Name
--- | ---
1 | Control Valve Channel Upper Plate Assembly Tip Inspect the upper channel plate bolt pass through holes for damage or burnelling. Any damage near the PCS feed holes could cause leaking around the PCS switch seal. Replace as necessary.
2 | Control Valve Body Bolt M6 x 35 (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Hand tighten for alignment, then tighten in sequence, after all bolts are installed.

Tighten
12 N·m (9 lb ft)

3 | Control Valve Body Bolt M6 x 65 (Qty: 5)

#### Procedure

Tighten in sequence.

Tighten
12 N·m (9 lb ft)

4 | Control Valve Body Bolt M6 x 55 (Qty: 2)

#### Procedure

Tighten in sequence.

Tighten
12 N·m (9 lb ft)