For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the HVAC Module. Refer to HVAC Module Assembly Replacement.
2. Remove Thermal Expansion Valve (TXV). Refer to Air Conditioning Evaporator Thermal Expansion Valve Replacement.

1 | Evaporator Upper Case Screw (Qty: 17) Caution: Refer to Fastener Caution in the Preface section. Tighten 6 N·m (53 lb in)
2 | Evaporator Upper Case
3 | Evaporator Core Tip Ensure all seals are in place upon installation.