For 1990-2009 cars

## Rear Seat Belt Buckle Replacement With 40 Percent

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement

1 | Passenger Seat Belt Buckle Caution: Refer to Fastener Caution in the Preface section. Tip Seat belt buckle and bolt are serviced as a assembly. Tighten
53 N·m (39 lb ft)

## Rear Seat Belt Buckle Replacement With 60 Percent

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the second row seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement.

1 | Rear Seat Belt Buckle Caution: Refer to Fastener Caution in the Preface section. Tip Seat belt buckle and bolt are serviced as a assembly. Tighten
53 N·m (39 lb ft)