For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat. Refer to Bucket Seat Replacement.

1 | Front Heated Seat Module Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Heated Seat Module

#### Procedure

• | Disconnect the electrical connector.

• | If a replacement module is installed, program the module. Refer to Control Module References.