For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the Instrument Panel Insulator Panel Replacement. Refer to Instrument Panel Insulator Panel Replacement - Left Side
2. Remove the Air cleaner. Refer to Air Cleaner Assembly Replacement .
3. Remove the Hood Primary and Secondary Latch. Refer to Hood Primary and Secondary Latch Replacement

1 | Hood Latch Release Cable

#### Procedure

1. Attach mechanic's wire to the existing cable at the latch side to ease installation of the new cab
2. Remove cable by pulling through the dash panel from inside the vehicle.