For 1990-2009 cars

## Instrument Panel Insulator Panel Replacement - Right Side Acadia

Callout | Component Name
--- | ---
1 | Push-pin Fasteners (Qty: 2)
2 | Insulator/Closeout Panel - Right

#### Procedures

1. Disconnect the electrical connectors.
2. Ensure the tab on the right side of the insulator locks into the carrier assembly securing the insulator to the instrument panel.

## Instrument Panel Insulator Panel Replacement - Right Side Enclave

Callout | Component Name
--- | ---
1 | Push-pin Fasteners (Qty: 2)
2 | Insulator/Closeout Panel - Right

#### Procedures

1. Disconnect the electrical connectors.
2. Ensure the tab on the right side of the insulator locks into the carrier assembly securing the insulator to the instrument panel.

## Instrument Panel Insulator Panel Replacement - Right Side OUTLOOK

Callout | Component Name
--- | ---
1 | Push-pin Fastener (Qty: 2)
2 | Insulator/Closeout Panel - Right

#### Procedure

1. Disconnect the electrical connectors.
2. Ensure the tab on the right side of the insulator locks into the carrier assembly securing the insulator to the instrument panel.

## Instrument Panel Insulator Panel Replacement - Right Side Traverse

Callout | Component Name
--- | ---
1 | Push-pin Fasteners (Qty: 2)
2 | Insulator/Closeout Panel - Right

#### Procedures

1. Disconnect the electrical connectors.
2. Ensure the tab on the right side of the insulator locks into the carrier assembly securing the insulator to the instrument panel.