For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the turn signal switch bracket. Refer to Turn Signal Switch Bracket Replacement.

1 | Ignition and Start Switch Housing Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
2 | Ignition and Start Switch Housing Strap
3 | Ignition and Start Switch Housing

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Transfer any parts as needed.