For 1990-2009 cars

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement.
2. Remove the engine flywheel bolts and flywheel. Refer to Engine Flywheel Removal.
3. Clean and inspect the flywheel. Refer to Engine Flywheel Cleaning and Inspection. If the flywheel teeth are damaged, inspect the starter for proper operation. Replace the starter if you find excessive wear or damage to the starter drive. Refer to Starter Motor Replacement.

### Installation Procedure

1. Install the engine flywheel and bolts. Refer to Engine Flywheel Installation.
2. Install the transmission. Refer to Transmission Replacement.