For 1990-2009 cars

## Front Bumper Fascia Brace Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the headlamp. Refer to Headlamp Replacement.
2. Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Bumper Fascia Brace Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft).
2 | Front Bumper Fascia Brace Nut Tighten 9 N·m (80 lb in).
3 | Fender Bumper Fascia Brace

## Front Bumper Fascia Brace Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Bumper Fascia Brace Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Front Bumper Fascia Brace Nut Tighten 9 N·m (80 lb in)
3 | Fender Bumper Fascia Brace