For 1990-2009 cars

## Driver or Passenger Seat Cushion Ventilation Heating and Cooling Blower Replacement Seat Back-Acadia, Enclave, Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat back cushion cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.

1 | Driver Seat and Passenger Seat Cushion Ventilation Heating and Cooling Blower

#### Procedure

1. Disconnect any electrical connectors.
2. Transfer components as necessary.

## Driver or Passenger Seat Cushion Ventilation Heating and Cooling Blower Replacement Seat Lower-Acadia, Enclave, Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement.

1 | Driver Seat and Passenger Seat Cushion Ventilation Heating and Cooling Blower

#### Procedure

Transfer components as necessary..

Tip
Note the new harness routing runs along the same path, but instead of clipping the harness to the top of the flex mat wire, clip the harness to the bottom of the flex mat wire. This eliminates the opportunity for the occupant loading to pinch the harness between the foam and the flex mat wire.